# Packet.h File Reference

`#include "win_bpf.h"`

Go to the source code of this file.

## Data Structures
struct | packet_file_header
| Header of a libpcap dump file. More...
struct | sf_pkthdr
| Header associated to a packet in the driver's buffer when the driver is in dump mode. Similar to the bpf_hdr structure, but simpler. More...
struct | _PACKET_OID_DATA
| Structure containing an OID request. More...
struct | _INTERNAL_REQUEST
| Stores an OID request. More...
struct | _PACKET_RESERVED
| Contains a NDIS packet. More...
struct | _DEVICE_EXTENSION
| Port device extension. More...
struct | __CPU_Private_Data
| Kernel buffer of each CPU. More...
struct | _OPEN_INSTANCE
| Contains the state of a running instance of the NPF driver. More...
struct | PacketHeader
| Structure prepended to each packet in the kernel buffer pool. More...
## Defines
#define | MAX_REQUESTS 32
| Maximum number of simultaneous IOCTL requests.
#define | Packet_ALIGNMENT sizeof(int)
| Alignment macro. Defines the alignment size.
#define | Packet_WORDALIGN(x) (((x)+(Packet_ALIGNMENT-1))&~(Packet_ALIGNMENT-1))
| even multiple of Packet_ALIGNMENT.
#define | KERNEL_EVENT_NAMESPACE L"\\BaseNamedObjects\\"
#define | MODE_CAPT 0x0
| Capture working mode.
#define | MODE_STAT 0x1
| Statistical working mode.
#define | MODE_MON 0x2
| Kernel monitoring mode.
#define | MODE_DUMP 0x10
| Kernel dump working mode.
#define | IMMEDIATE 1
| Immediate timeout. Forces a read call to return immediately.
#define | NDIS_FLAGS_SKIP_LOOPBACK_W2K 0x400
| This is an undocumented flag for NdisSetPacketFlags() that allows to disable loopback reception.
#define | TCPDUMP_MAGIC 0xa1b2c3d4
| Libpcap magic number. Used by programs like tcpdump to recognize a driver's generated dump file.
#define | PCAP_VERSION_MAJOR 2
| Major libpcap version of the dump file. Used by programs like tcpdump to recognize a driver's generated dump file.
#define | PCAP_VERSION_MINOR 4
| Minor libpcap version of the dump file. Used by programs like tcpdump to recognize a driver's generated dump file.
#define | NPF_DISABLE_LOOPBACK 1
| Tells the driver to drop the packets sent by itself. This is usefult when building applications like bridges.
#define | NPF_ENABLE_LOOPBACK 2
| Tells the driver to capture the packets sent by itself.
#define | C_ASSERT(a)
#define | RESERVED(_p) ((PPACKET_RESERVED)((_p)->ProtocolReserved))
| Macro to obtain a NDIS_PACKET from a PACKET_RESERVED.
#define | TRANSMIT_PACKETS 256
| of packets that can be transmitted at the same time or with a single call to NdisSendPackets.
#define | EXIT_SUCCESS(quantity)
| Macro used in the I/O routines to return the control to user-mode with a success status.
#define | EXIT_FAILURE(quantity)
| Macro used in the I/O routines to return the control to user-mode with a failure status.
## Typedefs
typedef struct _PACKET_OID_DATA | PACKET_OID_DATA
| Structure containing an OID request.
typedef struct _PACKET_OID_DATA * | PPACKET_OID_DATA
typedef struct _INTERNAL_REQUEST | INTERNAL_REQUEST
| Stores an OID request.
typedef struct _INTERNAL_REQUEST * | PINTERNAL_REQUEST
typedef struct _PACKET_RESERVED | PACKET_RESERVED
| Contains a NDIS packet.
typedef struct _PACKET_RESERVED * | PPACKET_RESERVED
typedef struct _DEVICE_EXTENSION | DEVICE_EXTENSION
| Port device extension.
typedef struct _DEVICE_EXTENSION * | PDEVICE_EXTENSION
typedef struct __CPU_Private_Data | CpuPrivateData
| Kernel buffer of each CPU.
typedef struct _OPEN_INSTANCE | OPEN_INSTANCE
| Contains the state of a running instance of the NPF driver.
typedef struct _OPEN_INSTANCE * | POPEN_INSTANCE
## Enumerations
enum | ADAPTER_BINDING_STATUS { ADAPTER_UNBOUND, ADAPTER_BOUND, ADAPTER_UNBINDING }
## Functions
| C_ASSERT (sizeof(PACKET_OID_DATA)==12)
NTSTATUS | DriverEntry (IN PDRIVER_OBJECT DriverObject, IN PUNICODE_STRING RegistryPath)
| The initialization routine of the driver.
PWCHAR | getAdaptersList (VOID)
| Returns the list of the MACs available on the system.
PKEY_VALUE_PARTIAL_INFORMATION | getTcpBindings (VOID)
| Returns the MACs that bind to TCP/IP.
BOOLEAN | NPF_CreateDevice (IN OUT PDRIVER_OBJECT adriverObjectP, IN PUNICODE_STRING amacNameP)
| Creates a device for a given MAC.
NTSTATUS | NPF_Open (IN PDEVICE_OBJECT DeviceObject, IN PIRP Irp)
| Opens a new instance of the driver.
VOID | NPF_OpenAdapterComplete (IN NDIS_HANDLE ProtocolBindingContext, IN NDIS_STATUS Status, IN NDIS_STATUS OpenErrorStatus)
| Ends the opening of an adapter.
NTSTATUS | NPF_Cleanup (IN PDEVICE_OBJECT DeviceObject, IN PIRP Irp)
| Closes an instance of the driver.
NTSTATUS | NPF_Close (IN PDEVICE_OBJECT DeviceObject, IN PIRP Irp)
VOID | NPF_CloseAdapterComplete (IN NDIS_HANDLE ProtocolBindingContext, IN NDIS_STATUS Status)
| Ends the closing of an adapter.
NDIS_STATUS | NPF_tap (IN NDIS_HANDLE ProtocolBindingContext, IN NDIS_HANDLE MacReceiveContext, IN PVOID HeaderBuffer, IN UINT HeaderBufferSize, IN PVOID LookAheadBuffer, IN UINT LookaheadBufferSize, IN UINT PacketSize)
| Callback invoked by NDIS when a packet arrives from the network.
VOID | NPF_TransferDataComplete (IN NDIS_HANDLE ProtocolBindingContext, IN PNDIS_PACKET Packet, IN NDIS_STATUS Status, IN UINT BytesTransferred)
| Ends the transfer of a packet.
VOID | NPF_ReceiveComplete (IN NDIS_HANDLE ProtocolBindingContext)
| Callback function that signals the end of a packet reception.
NTSTATUS | NPF_IoControl (IN PDEVICE_OBJECT DeviceObject, IN PIRP Irp)
| Handles the IOCTL calls.
VOID | NPF_RequestComplete (IN NDIS_HANDLE ProtocolBindingContext, IN PNDIS_REQUEST pRequest, IN NDIS_STATUS Status)
| Ends an OID request.
NTSTATUS | NPF_Write (IN PDEVICE_OBJECT DeviceObject, IN PIRP Irp)
| Writes a raw packet to the network.
INT | NPF_BufferedWrite (IN PIRP Irp, IN PCHAR UserBuff, IN ULONG UserBuffSize, BOOLEAN sync)
| Writes a buffer of raw packets to the network.
VOID | NPF_WaitEndOfBufferedWrite (POPEN_INSTANCE Open)
| Waits the completion of all the sends performed by NPF_BufferedWrite.
VOID | NPF_SendComplete (IN NDIS_HANDLE ProtocolBindingContext, IN PNDIS_PACKET pPacket, IN NDIS_STATUS Status)
| Ends a send operation.
VOID | NPF_ResetComplete (IN NDIS_HANDLE ProtocolBindingContext, IN NDIS_STATUS Status)
| Ends a reset of the adapter.
VOID | NPF_Status (IN NDIS_HANDLE ProtocolBindingContext, IN NDIS_STATUS Status, IN PVOID StatusBuffer, IN UINT StatusBufferSize)
| Callback for NDIS StatusHandler. Not used by NPF.
VOID | NPF_StatusComplete (IN NDIS_HANDLE ProtocolBindingContext)
| Callback for NDIS StatusCompleteHandler. Not used by NPF.
VOID | NPF_Unload (IN PDRIVER_OBJECT DriverObject)
| Function called by the OS when NPF is unloaded.
NTSTATUS | NPF_Read (IN PDEVICE_OBJECT DeviceObject, IN PIRP Irp)
| Function that serves the user's reads.
NTSTATUS | NPF_ReadRegistry (IN PWSTR *MacDriverName, IN PWSTR *PacketDriverName, IN PUNICODE_STRING RegistryPath)
| Reads the registry keys associated woth NPF if the driver is manually installed via the control panel.
NTSTATUS | NPF_QueryRegistryRoutine (IN PWSTR ValueName, IN ULONG ValueType, IN PVOID ValueData, IN ULONG ValueLength, IN PVOID Context, IN PVOID EntryContext)
| Function used by NPF_ReadRegistry() to quesry the registry keys associated woth NPF if the driver is manually installed via the control panel.
VOID | NPF_BindAdapter (OUT PNDIS_STATUS Status, IN NDIS_HANDLE BindContext, IN PNDIS_STRING DeviceName, IN PVOID SystemSpecific1, IN PVOID SystemSpecific2)
| Callback for NDIS BindAdapterHandler. Not used by NPF.
VOID | NPF_UnbindAdapter (OUT PNDIS_STATUS Status, IN NDIS_HANDLE ProtocolBindingContext, IN NDIS_HANDLE UnbindContext)
| Callback for NDIS UnbindAdapterHandler.
NTSTATUS | NPF_OpenDumpFile (POPEN_INSTANCE Open, PUNICODE_STRING fileName, BOOLEAN append)
| Creates the file that will receive the packets when the driver is in dump mode.
NTSTATUS | NPF_StartDump (POPEN_INSTANCE Open)
| Starts dump to file.
VOID | NPF_DumpThread (PVOID Open)
| The dump thread.
NTSTATUS | NPF_SaveCurrentBuffer (POPEN_INSTANCE Open)
| Saves the content of the packet buffer to the file associated with current instance.
VOID | NPF_WriteDumpFile (PFILE_OBJECT FileObject, PLARGE_INTEGER Offset, ULONG Length, PMDL Mdl, PIO_STATUS_BLOCK IoStatusBlock)
| Writes a block of packets on the dump file.
NTSTATUS | NPF_CloseDumpFile (POPEN_INSTANCE Open)
| Closes the dump file associated with an instance of the driver.
BOOLEAN | NPF_StartUsingBinding (IN POPEN_INSTANCE pOpen)
VOID | NPF_StopUsingBinding (IN POPEN_INSTANCE pOpen)
VOID | NPF_CloseBinding (IN POPEN_INSTANCE pOpen)
BOOLEAN | NPF_StartUsingOpenInstance (IN POPEN_INSTANCE pOpen)
VOID | NPF_StopUsingOpenInstance (IN POPEN_INSTANCE pOpen)
VOID | NPF_CloseOpenInstance (IN POPEN_INSTANCE pOpen)
NTSTATUS | NPF_GetDeviceMTU (IN POPEN_INSTANCE pOpen, IN PIRP pIrp, OUT PUINT pMtu)
UINT | GetBuffOccupation (POPEN_INSTANCE Open)
| Returns the amount of bytes present in the packet buffer.
## Variables
ULONG | g_NCpu
NDIS_HANDLE | g_NdisProtocolHandle
struct time_conv | G_Start_Time
UINT | g_SendPacketFlags

documentation. Copyright (c) 2002-2005 Politecnico di Torino. Copyright (c) 2005-2009 CACE Technologies. All rights reserved.