                                                                                                                        Copyright © 1996 Digital Equipment Corporation                             1

 AlphaServer 300 Release Notes

 EK AS300 RN. A01

   December 1996

     Setting Up Partitions for a Windows NT Server Installation

                                If you are installing the Windows NT operating system on a disk that has not been

                                partitioned and formatted, follow the procedure below.  These instructions supercede the

                                procedure documented in Appendix C of the AlphaServer 300 User’s Guide .

                                1. If the ARC console is running, go to step 2.  If the SRM console is running, type the

                                             following at the >>>  prompt:

                                             >>>set os_type nt

                                             Cycle the system power.  The system will restart with the ARC console running.

                                2. Insert the Microsoft Windows NT CD-ROM into the CD drive.

                                3. From the ARC console Boot menu, select Run a Program .

                                4. At the prompt, type:

                                             cd:\alpha\arcinst

                                             If you see receive a "Pathname is not defined" error, go to the ARC console Setup

                                             menu and select Set the environment variables.  Select CD-ROM , then

                                             enter the SCSI bus number and ID of the CD-ROM drive.  Next, select Set the

                                             default configuration  and follow the steps.  Save the changes and repeat

                                             step 4.

                                5. Choose

                                             Configure Partitions

AlphaServer 300 Release Notes

                                                          2

                             6. Choose

                                          Create Partition.

                                          A list of available target devices displays.

                                          Scsi bus 0,Identifier 0,Disk 0 (scsi(0)disk(0)rdisk(0))

                                          Identifier is the ID of the SCSI device, drive 0 in this case.  If partitions already exist

                                          on the target disk, select
                                                                                                                Delete Partition

 from the Configure Partitions menu.

                                          Follow the prompts and delete all the partitions on the disk.

                             7. Select the desired target device.  The system partition should be 6 MB, so enter the

                                          desired partition size of your C: drive minus 6 MB.

                                          Enter size in MB (1-1001): 995

                             8. Press any key to continue.  Enter n  at the following prompt:

                                          Do you want to make this the system partition (y/n)?   n

                                          Formatting scsi(0)disk(0)rdisk(0)partition(1)

                             9. Press any key to continue.  Choose

                                          Create System Partition

                                          A list of available target devices displays.

                             10. Select the desired target device. A prompt for partition size displays.

                             11. Enter 6 MB as the desired partition size of your D: drive:

                                          Enter size in MB (1-6): 6

                             12. Press any key to continue.  The following appears:

                                          Formatting scsi(0)disk(0)rdisk(0)partition(2)

                             13. Press any key to continue.  The Configure Partitions  menu redisplays.

                             14. Select Exit. The ARCINST menu displays.

                             15. Select Exit. The ARC Boot menu displays.

AlphaServer 300 Release Notes

3

16. Choose Supplementary Menu . . ., then choose Set up the syste m. . . .

               __________________________ Note _____________________________

                 It any items on the Setup menu are highlighted in yellow, address those items

                 before proceeding.  For example, you might need to set the system time.

               ________________________________ ____________________________

17. From the Setup menu choose  Edit environment variables .

18. At the  Name:  prompt, enter the following:

            Name:  systempartition

            The following value is displayed:

            scsi(0)disk(0)rdisk(0)partition(1)

            ;scsi(0)disk(0)rdisk(0)partition(2)

19. Press Home to go to the beginning of the line.  Using the Backspace key, delete the

            variable that ends with partition (1), including the semicolon:

            scsi(0)disk(0)rdisk(0)partition(1);

            You should now see only the following value:

            scsi(0)disk(0)rdisk(0)partition(2)

20. At the
                               Name:

                                                        prompt, press Esc to return to the Setup menu
.

21. From the Setup menu, choose Supplementary menu, and save changes . . .

22. Verify that the system partition is set correctly as follows:

            Return to the Setup menu and choose  Edit Environment variables.

            At the  Name: prompt, type  systempartition.   The following should be

            displayed:

            scsi(0)disk(0)rdisk(0)partition(2)

            Press Esc to return to the Setup menu, then choose
 Supplementary menu and

            do not save changes.

            You are now ready to install Windows NT.