  Multiple NICs and IP Addresses, No Routing? 
 The Question is:
 
How can I configure TCP/IP Services 5.0 to use two existing network controllers
 to connect the OpenVMS host to two different networks?
 
Now the second interface and dynamic routing are not configured, and the host
 should not route traffic between the two networks. Both networks are connected
 to Internet.
 
I tought that both interfaces should at least have their own IP address, mask,
 default gateway and also host and internet domain names. I looked at
 TCPIP$CONFIG, but couldn't find out, whether this is possible or not?
 
 
 The Answer is:
 
  OpenVMS TCP/IP Services generally assumes that routing is operating,
  particularly when multiple controllers (NICs) are present.
 
