  Why does OpenVMS report the wrong VAX system type? 
 The Question is:
 
We have a MicroVax 3100/98 equipped with Vms 6.2,
Mailworks, Message Router and PMDF that is used
as company Mail server.
 
When the computer startup I can read on system
console its identity as 3100/98.
 
Once that the computer is running the operating
system answer always that it is a 3100/95.
 
I have checked on DEC System Options that
the minimum VMS version for 3100/98 is 6.2.
 
I have ask to several VMS "experts" the reason
of the identity mismatch but I have received
only generic answers that all is ok.
 
I am worried about the situation because I have
never seen, before today, a Vax not perfectly
recognized by the proper version of VMS.
 
I suspect that in this situation VMS don't use
properly the HW and the VPA don't give a proper
analysis of system load and performances.
 
It is necessary to apply any patches to VMS
or to Hw firmware ?
 
Thank you.
 
Salvatore Longobardo - Marconi Communications spa
 
 
 The Answer is:
 
  As you have been told: all is OK.
 
  The newer VAX systems are explicitly designed to closely emulate older
  VAX systems, systems that were supported by older OpenVMS releases.
  Because of this explicit emulation, the specific system type of the newer
  system will be misidentified as an older (and supported) system type.
  This is known, expected, and entirely correct behaviour when using one
  of these older OpenVMS VAX releases, albiet confusing.
 
  Unlike recent Alpha systems and the OpenVMS Alpha operating system, VAX
  systems and OpenVMS VAX software lack support for the feature known as
  Dynamic System Recognition (DSR).  DSR allows the operating system to
  directly query the system for information such as the text-format system
  name and other necessary system-specific information.  Without DSR, there
  is no way for an existing OpenVMS VAX release to (uniquely) identify a
  newer VAX system, as this knowledge must be built into the OpenVMS VAX
  release.  Building this platform knowledge into the OpenVMS VAX release
  would require a new release, and would mean that you must upgrade to a
  more recent OpenVMS VAX version for support.  Building DSR into OpenVMS
  VAX would require both hardware and software updates, and no support for
  DSR is planned for OpenVMS VAX or any VAX platforms.
 
  The alternative to requiring the OpenVMS upgrade for new hardware support,
  or to adding DSR into OpenVMS VAX and VAX hardware, is for the new VAX
  hardware to closely emulate an existing older (and supported) VAX system.
  This is (obviously) the particular behaviour you see.
 
  As you upgrade to newer OpenVMS VAX releases, there are generally "clues"
  left in the VAX hardware that allow the software to identify a particular
  variant of the (known) platform.  These clues mean that (eventually) an
  OpenVMS VAX release can be altered to display the correct system type.
 
