  OpenVMS LPD_UNPRTR? 
 The Question is:
 
I have a failure of an Hp3000 mpe system to print to vms with the lpr system.
The log message is :
ACP AUXS error during process exit
Status= %UCX-F-LPD_UNPRTR
 
Can I turn on any better debugging to see what happened??
 
 
 The Answer is:
 
  Please see the various existing discussions of LPR printing,
  as well as the available TCP/IP Services documentation.
 
  Also please consider direct contact with the Compaq Customer
  Support Center, as this may well involve some research and
  probably some additional information to resolve.
 
  As a start, please acquire the current ECO kit for whichever
  version of TCP/IP Services is in use -- V4.2 with the current
  ECO would be the appropriate choice here.
