  TCP/IP (UCX) SET SERVICE returns INVRECORD? 
 The Question is:
 
We are running UCX 4.0 on VAX VMS 5.5-2 (yes I
know it's not supported).  When I try to add a
network ip to the "accept" list using the
command:
 
UCX&gt; set service telnet/accept=networks=(network)
 
I get the message
 
%UCX-E-INVRECORD, Invalid information
 
Is there any hope for me?
 
 
 The Answer is:
 
  TCP/IP Services for OpenVMS V4.0 ECO 3 (and later) include a fix for this.
