  Cluster Communications via multiple LANs? 
 The Question is:
 
If I have a two node lavc cluster, with each machine having two interfaces, one
 FDDI, and one Ethernet, and all interfaces connected to the same translational
 bridge, will they still cluster if the FDDI interface on one machine is
 disabled and the Etherne
t interface on the other machine is disabled?
 
I find through testing, removing FDDI connection on one machine and the
 Ethernet connection on the other machine, that they will not. Is there a way
 to make it work?
 
 The Answer is:
 
  Please contact the organization that is supporting your bridge, as
  it appears that it is not forwarding network packets as you expect.
 
