  TCP/IP (UCX) PPP; OpenVMS client dial-out? 
 The Question is:
 
DecServer 900 &amp; PPP
 
I have read all the documentation I can get my hands on regarding supporting
PPP access to an alpha server with UCX 4.2 using a DecServer. I believe that
I can manage to configure the system to allow clients to access the alpha
through the decserver. Howe
ver, what I really want to do is have the alphaserver as the client side of
the connection. (The server side would be a Windows NT RAS server). Is this
possible, and if so, can you point me in the right direction.
Regards,
Jim Windram,
Nissan UK.
 
 The Answer is:
 
  If the information in the documentation set and specifically the
  information in the OpenVMS file:
 
    SYS$COMMON:[SYSHLP.EXAMPLES.PPPD.DOC]PPPD_CONNECT.TXT
 
  is insufficient for your needs, and you have checked previous PPP
  discussions here, please contact the customer support center directly.
 
 
