  TCP/IP (UCX) telnet printing to HP? 
 The Question is:
 
I am trying to print a file to a TCP/IP UCX queue.
The printout do not show the last 10 caracters or so.
 
We think that the problem comes from a predetermine
page with but we can't find were to set it.
 
Here is our UCX queue initialization.
$! INITIALIZE EXECUTION QUEUE HP1
$ init/queue/start-
                /owner=[1,4]-
                /retain=error-
                /device=server-
                /process=ucx$telnetsym-
                /default=(nofeed)-
                /library=hp_devctl -
                /separate=(noflag,reset=(hp_reset)) -
                /on="hp1:9100"-
                /protection=(s:e,g:r,w:w,o:d) HP1
 
Thank you for your help !
 
Marc-Alain
 
 The Answer is:
 
  Please contact the customer support center.  Expect to be asked about
  the TCP/IP Services for OpenVMS (UCX) version, as well as any UCX ECO
  kits that have been applied, as well as the type of HP Printer.
