  HSJ Mirrorset RAID Controller Maintenance? 
 The Question is:
 
How do I replace a deffective disk in a Controller based Mirrorset. The
 replacement disk has been added to the cabinet but I need to add it to the
 mirrorset without losing the information on DISK500
 
Note: DISK500 is the 'REDUCED' disk
 
HSJ02&gt;show mirror2
Name          Storageset                     Uses             Used by
------------------------------------------------------------------------------
 
MIRROR2       mirrorset                      DISK500          D500
        Switches:
          NOPOLICY (for replacement)
          COPY (priority) = NORMAL
          READ_SOURCE = LEAST_BUSY
          MEMBERSHIP = 2, 1 member present
        State:
          REDUCED
          DISK500   (member  0) is NORMAL
        Size: 8378028 blocks
 
Thank you,
 
Bert
 
 The Answer is :
 
  Please contact your hardware support organization for assistance with
  system maintenance and repair -- details on the specific model of HSJ,
  the firmware and the configuration will be required.  (The OpenVMS
  Wizard is also not particularly familiar with VAX controller-based
  RAID hardware, nor with controller reconfiguration requirements.)
 
 Answer written or last revised on  25-NOV-2002 
