  More TCP/IP (UCX) telnet logins? 
 The Question is:
 
   Is UCX limited in the number of connections?  If not how can I increase
the number of concurrent connection?  If it is a SYSGEN parameter which
one(s)?
 
  After approximatly 60 successful remote telnet terminal emulation logins,
additional remote login attempts are not greeted with usual username:
request.  At this point, if I have the user switch protocol to LAT or DECnet
he/she can login no problem.
 
 
  My goal is to have a pure TCP/IP network and standardize and simplify my
desktop configurations.  I know a solution exist please help.  Note: if the
answer is in the UCX documentaion I can not find it!
 
  I am currently running OpenVMS V7.1-1H1 and UCX V4.1-12 with UCXECO_41_2
V2.0.
 
Thanks,
John
 
 
 The Answer is:
 
  SET LOGINS/INTERACTIVE is one obvious limit, the number of processes
  permitted by MAXPROCESSCNT is another, as are the TCP/IP Services for
  OpenVMS (UCX) communication services limits set by the UCX command SET
  COMMUNICATION /SERVICES.
 
