  LATCP SET PORT command failure? 
 The Question is:
 
Do you have a fix for this?
 
 The Answer is :
 
  Assuming this isn't simply an erroneous SET PORT command,
  please contact the customer support center.  (As shown, the
  SET PORT erroneously targets two devices, LTA1: and LTA10:.
  Please pick exactly one target device for the SET PORT.)
 
 Answer written or last revised on  4-FEB-2002 
