  Cluster Satellite Failure, unknown NIC? 
 The Question is:
 
boooting a DS25E satellite:
 
hello,
 
i want to boot a DS25E cluster satellite node over the ethernet. (bootserver is
 a ident DS25E boot server).
 
when I boot from the 10/100 Mbit board EIA0, everything is ok.
when I boot from the 10/100/1000 Mbit board EGA0, it did not work.
 
console messages: EGA0  - does not work
 
P00&gt;&gt;&gt;boot ega0
(boot ega0.0.0.5.2 -flags 0,0)
 
Trying MOP boot.
..........
 
Network load complete.
336 Packets, Max pkt size 1492, Retries 0
Loaded by: aa-00-04-00-91-7d
Host name: LVS001
bootstrap code read in
base = 714000, image_start = 0, image_bytes = 792c5(496325)
initializing HWRPB at 2000
initializing page table at 3fff0000
initializing machine state
setting affinity to the primary CPU
jumping to bootstrap code
%VMScluster-I-MOPSERVER, MOP server for downline was node LVS001
%SYSBOOT-I-QIOSERVER, Boot driver image name SYS$DKDRIVER.EXE
%VMScluster-I-REINIT_WAIT, Waiting for access to the system disk server
%VMScluster-I-REINIT_WAIT, Waiting for access to the system disk server
 
 
console messages: EIA0  - works fine
 
P00&gt;&gt;&gt;b
(boot eia0.0.0.8.0 -flags 0,0)
 
Trying MOP boot.
..........
 
Network load complete.
336 Packets, Max pkt size 1492, Retries 0
Loaded by: aa-00-04-00-91-7d
Host name: LVS001
bootstrap code read in
base = 714000, image_start = 0, image_bytes = 792c5(496325)
initializing HWRPB at 2000
initializing page table at 3fff0000
initializing machine state
setting affinity to the primary CPU
jumping to bootstrap code
%VMScluster-I-MOPSERVER, MOP server for downline was node LVS001
%SYSBOOT-I-QIOSERVER, Boot driver image name SYS$DKDRIVER.EXE
%EIA-I-BOOTDRIVER, Console setting is Fast
%EIA-I-BOOTDRIVER, Selected 100BaseTX HDX
 
kind regards
christian koessl
 
 
 
 
 The Answer is :
 
  Please contact the customer support center, as details of the cluster
  configuration and of the particular NIC will be required.
 
 Answer written or last revised on  21-NOV-2002 
