  IP Packet Size? 
 The Question is:
 
What is the packet size in the output of the
command ucx show interface/full or how is it
found?
 
 The Answer is :
 
  It is usually best to avoid encoding this knowledge into any
  application.
 
  For MTU-related information, see topics (825) and (6443), and
  also please see the discussions of Jumbo Frames in the OpenVMS
  documentation.  Jumbo Frames are part of OpenVMS Alpha V7.2
  and later releases.
 
 Answer written or last revised on  25-JUN-2003 
