  Translation of error 030AEBB4? 
 The Question is:
 
I have print queues which occasionally report a status of 030AEBB4 ( as seen
 using the command ACC/FULL/STATUS=030aebb4 )and prints fail to appear.  This
 is connected to multiple prints in quick succession, subsequent lower volumes
 of prints appear as nor
mal. The status does not have any associated message text but I suspect it is
 connected with UCX.  We are on version 4.1 ECO 2 of UCX.
Can you tell me what this status return means ?
 
 The Answer is:
Message found in SYS$COMMON:[SYSMSG]UCX$MSG.EXE;2
%UCX-F-LPD_NOSPOOLDIR, Error is spool directory !AS
 
  disk full perhaps?
