  SET HOST to HSG controllers? 
 The Question is:
 
Hello Wizard.
 
I'm trying to find a way to connect from DCL to our HSG controllers.
 Previously, we've used set host/dup/server=...... to connect to HSD/J
 controllers. In Tru64, one can connect to the GGA device presented by the HSG
 to the operating system. How does one
do this from DCL ?
 
many thanks,
 
Nick.
 
 
 The Answer is:
 
  Software for the purpose of interactive access to Fibre Channel storage
  controllers is available from the Compaq Customer Support Center.
 
