  Multi-host SCSI Enclosure Support? 
 The Question is:
 
Hi;
 
I am familiar with shared SCSI OpenVMS clusters using FWD controllers (KZPBA)
 and differential BA356 shelves.
 
Can I use an Alpha LVD controller with either 4200 or 4300 series shelves in a
 similar configuration or is this not supported?  This provides universal drive
 compatibility which is a big issue for me. I could not find an specific
 references one way or the
 other.
 
Any help appreciated.
 
Chris Butler
 
 The Answer is:
 
  The list of controllers supported for multi-host operations is
  included in the OpenVMS Cluster SPD and the Cluster documentation.
 
  The OpenVMS Wizard is aware of OpenVMS Cluster multi-host SCSI
  configurations using the "universal" SCSI devices.
 
