  DEMSA SNA Gateway? 
 The Question is:
 
DEMSA-AA used as DEC SNA Gateway ST with one
line configured (SYN-1) needs speed updated
from 9600 to 19200 for FEP connection. I believe I recall that there is
 configuration work to be done in the DEMSA, but cannot find hide nor hare of
 the way to tell these lines what speed they operate at. Are they auto-baud
lines? SYN-1 connected via v.35 cable to CSU/DSU.
 
 
 
 The Answer is:
 
  The DEMSA was retired many years ago, and was last in common
  use roughly a decade ago.
 
  The usual mechanism for widgets of this vintage was to set the
  output line speed via NCL command.
 
  Common commands:
 
 
create modem connect line dte-1 communication port syn-0-1, profile  "NORMAL"
set modem connect line dte-1 speed 19200
set modem connect line dte-1 modem control full
set modem connect line dte-1 suppress test indicator true
 
