  Configuring a Modem on OpenVMS? 
 The Question is:
 
How should I cofigure TTA port to connect to my OpenVMS instalation via dial-up
 line (from PowerTerm instlation on PC) ?
 
 
 The Answer is:
 
  Match up the capabilities of the local port with the communications
  capabilities and the requirements of the modem, and also remember to
  review the existing discussions of modems and of flow control here
  in the Ask The Wizard area.
 
  Some of the existing discussions of modems include the following:
 
    (81), (153), (271), (300), (364), (634), (1001), (1016), (1761),
    (1839), (1935), (2094), (2177), (2488), (2936), (2950), (2960),
    (3033), (3127), (3633), (3695), (3925), (4331), (4347), (4566),
    (4639), (5576), (5852), (5997), (6015), (6758).
 
  Various related topics are included in the OpenVMS FAQ.
 
