  Redundent Network Configuration? NetRAIN? 
 The Question is:
 
I would like to take advantage of the 2 Ethernet ports on my
 EX900s/ES40s/DS20Es for dual-home network connections to seperate switches in
 the network for redundancy. How do I configure the fail-over in software for
 the TCP/IP protocal?
 
 
 The Answer is :
 
  Configure the ports as normal, using the normal configuration tools.
 
  NetRAIN-like fail-over is not yet available on OpenVMS with TCP/IP
  Services, each NIC will have its own IP address.
 
 Answer written or last revised on  14-AUG-2002 
