  Defining an IP route? 
 The Question is:
 
How to set a route of 192.168.0.0/16 using the ucx set route/mask command?
 
 The Answer is :
 
  The SET ROUTE /MASK command would be the usual approach here.  As
  this is apparently malfunctioning, please ensure that you have a
  recent (V5.1) or current version (V5.3, as of this writing) and the
  current ECO, and please contact the support center for assistance.
 
 Answer written or last revised on  12-AUG-2002 
