  DNS/BIND configuration, failover? 
 The Question is:
 
Is there a way to set up two dns servers (one primary the other a failover) in
 UCX, similar to two entries you can make in NT and Unix? What would the UCX
 commands be?
 
Thanks,
 
Mike
 
 The Answer is :
 
  Please move to a current TCP/IP release, and please read the
  available documentation on configuring DNS and DNS failover.
  For pointers to the OpenVMS documentation, please see the FAQ.
 
 Answer written or last revised on  27-AUG-2002 
