  LAT and non-DECnet Ethernet addresses? 
 The Question is:
 
When LAT is starting up, how do I tell it
to use the real MAC address of the adapter
instead of the DECnet address that is bound
to that adapter?
 
Thanks.
 
 
 The Answer is:
 
  Please see the LATCP command CREATE LINK/[NO]DECNET for details.
