  LT and TN devices, LAT and Telnet Printing? 
 The Question is:
 
I am trying to setup a print queue using TCPIP$TELNETSYM.  The queue works
 fine, but I need to use a LTA device spooled to the queue.  The LTA device is
 not responding or working correctly.
 
 The Answer is :
 
  LT-class devices are LAT devices and are accordingly completely
  unrelated to IP and to TN-class IP telnet printing.
 
  LT-class devices use the standard OpenVMS print symbiont, not
  the telnet nor lpr/lpd symbionts.
 
  See (546), (1020), (1370), (1679), (1938), (2312), (2631), (2696),
  (3041), (3250), (3202), (3280), (4394), (5173), (5737), (5881),
  (6271), (6467), (7143), (7151), (7530), (7959), and other topic.
 
 
 Answer written or last revised on  13-DEC-2002 
