  DECserver port framing errors? 
 The Question is:
 
Decserver ds732 port framing errors. My question is when your server receives
 stupid amounts of framing errors is this generally a server problem or a
 config issue.
 
Network Access SW V2.4 BL50 for DS732     ROM V7.3-0  Uptime:  17 11:25:34
 
Address:   00-60-6D-22-21-0A   Name:   C-LABDSRV035       Number:     0
 
                     Cur  High  Max
Active Ports:         26    26   32     Minutes To Shutdown:        N/A
Active Users:         26    26   32     Discarded Nodes:              0
Queue Entries:         0     0  100     Resource Errors:              0
 
Available Services:    1     1  N/A     Port Framing Errors:     752606
Local Services:        0     0    0     Port Parity Errors:           0
Reachable Nodes:       1     2  200     Port Overrun Errors:          5
 
                                        Boot Device:       Flash RAM: 0
Active Circuits:       0     1   32     Primary Hosts:
Connected Nodes:       0     0   32     Load Address:
Connected Sessions:   13    18   64     Dump Address:    None Available
% CPU Used:           47   100  100     Console User:       10.249.4.47
% Memory Used:        17    17  100     Boot Protocol:
 
Selftest Status: Normal
Software Status: Normal
 
 The Answer is :
 
  Port framing errors imply a serial line baud (speed) mismatch between
  the DECserver port and the connected serial device, or a mismatch of
  stop bits or port characteristics.
 
  For assistance with the DECserver series device hardware, please
  contact the Digital Network Products Group at www.dnpg.com.
 
 
 Answer written or last revised on  2-APR-2003 
