  StorageWorks Controller Configuration? 
 The Question is:
 
Configuration  2 node DS20E  OpenVMS Cluster with one FC 64 bit adaptor(LP8000)
 in each node , one 8 port FC switch and a dual HSG80.
 
Is it possible to partition  a storageset  (on the HSG's) into more VMS disk
 units and still have HSG80 to HSG80 failover .
I do know the configuration has a single point of failure in the FC switch.
 
There seems to be a restriction for dual HSZ's here!
 
 
 
 
 The Answer is:
 
  Please contact the Compaq Customer Support Center, your Compaq reseller,
  or the local StorageWorks team for assistance with configuring the HSG
  series storage controllers.
 
