  DNS/BIND configuration for Active Directory? 
 The Question is:
 
What do I need to do to configure tcpip on VMS so that so that VMS is the
 primary DNS server for a Windows 2000 Active Directory?
 
 
 The Answer is :
 
  Please see the discussion of this topic at the Encompasserve website,
  (http://eisner.decus.org/), and specifically please look in conference
  EISNER::DEC_NETWORKING topic (1448).
 
 Answer written or last revised on  17-NOV-1858 
