  FDDI Packet Size via NCL? 
 The Question is:
 
Under NCL, how do I determine what the FDDI packet size is?   We run
multinet, not UCX, but I believe this parameter to be controlled with NCL.
 
Thanks!
 
 
 The Answer is:
 
 
  The DECnet NCL syntax should be similar to:
 
    'sho rou cir fddi* data link sdu size'
 
  The TCP/IP Services syntax should be similar to:
 
    'show interface wf0'
 
  Specifically check the output in the MTU column.
 
  There are slight differences expected in the numbers reported
  by the different packages, likely due to different overhead.
 
  As for MultiNet, please contact MultiNet support.
 
