  IP Configuration Database Corruption? 
 The Question is:
 
MicroVAX 3100, hardware model type 156
UCX V4.0
 
Error starting UCX:
%UCX-E-INETERROR, Error accessing Internet
-UCX-E-INVQUAL, Invalid qualifier value for /LOCAL_HOST
-RMS-E-RNF, record not found
 
Error Internet IVP:
Begin IVP...
%%% UCX IVP: started %%%
%%% UCX IVP: error - Local Host Not Found  %%%
%SYSTEM-F-NOLOGNAM, no logical name match
IVP request completed.
 
UCX&gt;Show Hosts
     LOCAL database
Host address    Host name
127.0.0.1       LOCALHOST, localhost
10.3.12.3       SMSD3, smsd3
.... and some more system.
smsd3 is the local system
 
UCX&gt;SHOW SERVICES
Service             Port  Proto    Process          Address            State
 
FTP                   21  TCP      UCX$FTPD         0.0.0.0             Enabled
LPD                  515  TCP      UCX$LPD          0.0.0.0             Disabled
MOUNT                 10  UDP      UCX$NFS          0.0.0.0             Enabled
NFS                 2049  UDP      UCX$NFS          0.0.0.0             Enabled
PCNFS               5151  TCP,UDP  UCX$PCNFSD       0.0.0.0             Enabled
PORTMAPPER           111  TCP,UDP  UCX$PORTM        0.0.0.0             Enabled
REXEC                512  TCP      UCX$REXECD       0.0.0.0             Disabled
RLOGIN               513  TCP      not defined      0.0.0.0             Enabled
RSH                  514  TCP      UCX$RSHD         0.0.0.0             Disabled
SMTP                  25  TCP      UCX$SMTP         0.0.0.0             Enabled
SNMP                 161  UDP      UCX$SNMP         0.0.0.0             Disabled
TELNET                23  TCP      not defined      0.0.0.0             Enabled
 
UCX&gt;SHOW INTERFACE
                                                           Packets
Interface   IP_Addr         Network mask          Receive          Send     MTU
 
 SE0        10.3.12.3       255.255.252.0           10058            49    1500
 LO0        127.0.0.1       255.0.0.0                   1             3   65535
 
It is not possible to reach this system with telnet or ping. I think this is a
 configuration problem? Many thanks for your help
 
 
 The Answer is :
 
  Re-configure and re-enable IP routing with UCX$CONFIG, as it appears
  that there is some sort of problem with the local configuration.  A
  missing or a corrupt file, or missing configuration data apparently
  lurks here.
 
  If you choose the following route, make CERTAIN you keep and archive
  copies of the files BEFORE you delete or rename them.   For a complete
  reconfiguration of TCP/IP Services, shut down IP, delete or rename all
  of the local system IP configuration data files (SYS$SYSTEM:UCX*.DAT),
  perform the UCX$CONFIG configuration, and start IP.
 
  Your OpenVMS VAX and TCP/IP Services versions are ancient and an
  upgrade is strongly recommended.  If you must operate on versions
  from 1992 or so, you will want to install the available (mandatory)
  ECO kits for both OpenVMS VAX and TCP/IP Services.
 
 Answer written or last revised on  18-JUN-2003 
