  RW Series Optical Jukebox? 
 The Question is:
 
What layered product is used to access the media changer on an RW504 optical
 jukebox?
 
I can init, mount, read/write and even boot from the media currently loaded in
 the drive, but I can only change media from the RW control panel.
The drive and changer show up as seperate SCSI id's.
 
VAXstation 3540 (hobbyist system)
Currently running VMS 5.5, but I will be upgrading to v7.
 
 The Answer is:
 
  OSMS was the package.
 
