  Ethernet CSMA-CD Carrier Check Failures? 
 The Question is:
 
carrier check failure from : Node LOCAL:.vmsy2k CSMA-CD station CSMACD-1,
at: 2000-06-01-14:08:09.305+08:00Iinf
 
 The Answer is :
 
  Your network hardware is reporting a network or hardware problem.
 
  Related topics include (7105), (3500), (3516), (3632), and (4439).
 
 Answer written or last revised on  8-NOV-2001 
