  Problems with telnet and eight-bit? 
 The Question is:
 
 
I upgraded from UCX 4.2 to UCX 5.0.
UCX SHOW VERSION reports 5.0
 
Now, some of our Telnet CLIENT apps do not run correctly. They require full
 8-bit binary mode and it appears that UCX is stripping out
some 8-bit values.
The telnet client app is definitely not seeing the 0xff value.
Again, this worked on UCX 4.2.
 
How do I fix this Telnet problem or tell the Telnet server to start up in 8-bit
 mode.
 
 The Answer is:
 
  Please use TCP/IP V5.0A.
 
  Please contact the Compaq Customer Support Center, as details of the
  client application and of the OpenVMS host terminal settings will be
  required.
 
