  Disabling secondary cache? 
 The Question is:
 
What are some of the causes of a: "sysloa670-e-nobc Disabling secondary cache
 error"
 
Thanks,
 
Jack Plain
 
 The Answer is :
 
  Hardware problems with your VAX 4000-300 system memory cache would
  be the most common cause of the specified error message.
 
  Please contact your hardware services organization for assistance.
 
  Related topics include (8062).
 
 Answer written or last revised on  13-JAN-2003 
