  Clustering and Allocation Classes? 
 The Question is:
 
I have DSSI disks on a VAX in a cluster with an Alpha.  The DSSI controllers
 and the VAX are all allocation class 2 (the Alpha is allocation class 1).
The SYSGEN parameter MSCP_LOAD=2 on all nodes, but the VAX DSSI devices do not
 show up on the Alpha.  Yet, some RRD40 devices on the VAX *do* show up on the
 Alpha. How can I get the VAX's DSSI devices to appear to the Alpha system?
 
 
 The Answer is :
 
  MSCP_LOAD controls the loading of the MSCP disk services.  MSCP_SERVE_ALL
  controls whether or not the disks are served to other cluster members.
  (The latter parameter is probably set to serve just local devices.)
 
 Answer written or last revised on  17-DEC-2003 
