  SCSI disk and tape jumper settings? 
 The Question is:
 
What do each of the jumpers on the back of a DEC RZ56-e disk memory unit do?
 
Specifically, which one(s) have it spin up after a delay or from a signal by
 the controller and not on startup?
 
Also is it SCSI 1 or 2 and is there a jumper to select between the two?
 
 The Answer is:
 
  Please see the available information on storage hardware that
  is referenced in the OpenVMS FAQ.
 
