  UDP Protocol quota settings? 
 The Question is:
 
Dear Wizard,
I'm using UCX 4.2 and I noticed this thing:
in the UCX documentation it is stated that the maximum value for the default
 UDP buffer quota is 128Kb, but I found I can set a larger value (i.e. 4000000)
 from the command line (UCX SET PROTOCOL UDP /QUOTA=REC=4000000) and it is
 accepted and used by the
system. My question is:
what's wrong, the documentation or UCX?
Thank you
 
 
 The Answer is:
 
  OpenVMS V7.2 does not and can not support TCP/IP Services V4.2.
 
  Please move to a version of TCP/IP Services supported with this
  OpenVMS release, specifically V5.0A (with ECO) or V5.1, or later.
 
  Please also check the documentation for the current release of
  TCP/IP Services -- the OpenVMS Wizard finds a listing for UDP,
  but no maximum size is specified in the documentation.
 
