  Seeks StorageWorks Wizard? 
 The Question is:
 
We have a 'new' TL895 (under contract) and have 4 tape drives in same although
 it came with no drives.  We moved 4 TZ89 drives from our TL894 initialized,
 calibrated, rebooted our MDR, ran sysman io Find_WWid, io auto. VMS sees the
 drives and they functio
n but the robot commands only see drive 0 not 0-3. How can we get the robot
 commands to work?  I've been told maybe we need to set the SCSI ids via the
 TL895 console but how?
 
 The Answer is :
 
  Please contact your hardware support organization for assistance with
  configuring this or other storage devices.
 
  (The OpenVMS Wizard is unfortunately not a StorageWorks Wizard.)
 
  Typically, the TL895 robot is set to SCSI unit 1, and each DLT tape
  drive present is configured to sequential (and contiguous) SCSI units
  starting at unit 2.
 Answer written or last revised on  12-JAN-2003 
