  Configuring IP Printing Services? 
 The Question is:
 
I'd like to know how to run LAT over a TCP/IP connection or else how to
create a Line Printer using TCP/IP (not queued)
 
 
 The Answer is:
 
  Protocols such as LAT and SCS operate directly over the network,
  and are not routed or encapsulated, and cannot be operated over
  DECnet or IP.
 
  For information on configuring printing services via LPR/LPD and
  Telnet, please see:
 
    http://www.openvms.digital.com:8000/72final/
       6526/6526profile_028.html#part6
 
  For information on the IP equivilent of the "reverse LAT" capability,
  please see the various previous "reverse" discussions here in the
  OpenVMS Ask The Wizard area.
 
