  Configuring IP Printers? 
 The Question is:
 
How do I set up a print queue for an HP Color Laser Jet printer using DHCP
commands?
 
 
 The Answer is:
 
  DHCP provides IP addresses, and OpenVMS requires TCP/IP Services
  V5.0 or later for DHCP Server support.  Support for DHCP Client
  capabilities for OpenVMS are planned for a future release of
  TCP/IP Services.
 
  For information on configuring printers using TCP/IP, please see
  the available information here in Ask The Wizard, as well as the
  existing TCP/IP Services documentation -- the TCP/IP Services
  documentation is available at the OpenVMS documentation website
  referenced in the OpenVMS FAQ.
 
