  Printer IP Port Assignment? 
 The Question is:
 
I have successfully built "telnet" (init/que/proc=ucx$telnetsym) print
queues to HP printers attached to our LAN via ExtendNet boxes (makes printer
an ethernet device with an IP address). I was told that the port number
(pertaining to the init/queue comma
nd, parameter /on="node:port") for HP printers is 9100. Where can I find out
what port number to use for other printers, for example a Genicom line
printer? Thank you!
 
 The Answer is:
 
  Please see topic 1020 for some related information.
 
  Please check the printer documentation, the printer setup page (if
  any), or ask the printer vendor for details on the particular port
  used by the printer.
