  Maximum Number of TCP/IP Device Sockets? 
 The Question is:
 
In UCX v4.2, I could enter the above command to see the maximum number of
 device_sockets.  In TCPIP v5.1, I do not get that information when I enter the
 same command.  What are the commands that I need to show and set the maximum
 number of device_sockets?
 
 
 The Answer is :
 
  The OpenVMS Wizard is not aware of an analog, as the internals of
  TCP/IP Services have changed.  The usual limits are that of the
  available system pool, and the configured total limit on sockets,
  and (depending on what you are up to) the channelcnt setting.
 
 Answer written or last revised on  29-MAR-2002 
