  Help decoding hardware error log? 
 The Question is:
 
Sirs,
 
We have an Vax 7000 system ,but recently it seem has some problems . I don,t
 know if it is about the memory's problem. The following is the error
 log.Please help me to find where the problem is.
Thank you.
 
 
 ******************************* ENTRY       3. *******************************
 ERROR SEQUENCE 38990.                           LOGGED ON:        SID 17000201
 DATE/TIME 30-JUN-2000 07:34:58.23                            SYS_TYPE 01420201
 SYSTEM UPTIME: 4 DAYS 18:21:08
 SCS NODE: TAIT                                                VAX/VMS V6.2
 
 INT60 ERROR KA7AA-AA  CPU FW REV# 1.  CONSOLE FW REV# 4.2
       PACKET REV      00000002
       RESERVED        00000000
 
       SW FLAGS        00008000
                       00000000
                       00060000
                       00000400
                                       LSB error log snapshot packet present
       LOGGING OFF     00000000
                       00000000
                       00000000
                       00000000
       ACTIVE CPUS     00000007
       HW REVISION     00000000
       SYS SERIAL NUM  00005651
                       00000000
                           0000
                                       SYS SERIAL NUM = QV........
       SERIAL NUMBER   30365941
                       35303336
                           3339
                                       SERIAL NUMBER = AY60630593
       RESRC DISABLE   00000000
 
       PHYS ADDRESS    F8400000
                       00000000
       LDEV            00028002
                                       Laser NVAX Processor, 4M
                                       Device Revision = 02(X)
       LBER            00040209
                                       ERROR LINE ASSERTED -----------
                                       CORRECTABLE DATA ERROR
                                       TRANSMITTER DURING ERROR
                                       NODE-SPECIFIC ERROR
       LCNR            00000001
                                       Enable Correctable Err Detection
                                       Self Test Passed
       LMERR           00000080
                  -------------------- B-CACHE DATA SINGLE BIT ERROR----------
       LMMR6           00000381
                                       Enable output
                                       interleaved modules = 1, compare bits 0
                                       Interleave Address = 00(X)
                                       Address Width = 0C(X)
                                       banks per mod = 2, bits in bank = 1
                                       Module address = 00000000(X)
       LMMR7           00100381
                                       Enable output
                                       interleaved modules = 1, compare bits 0
                                       Interleave Address = 00(X)
                                       Address Width = 0C(X)
                                       banks per mod = 2, bits in bank = 1
                                       Module address = 00000008(X)
       LBESR0          00000000
                                       Syndrome 0 = 00(X)
       LBESR1          00000070
                                       Syndrome 1 = 70(X)
       LBESR2          00000000
                                       Syndrome 2 = 00(X)
       LBESR3          00000000
                                       Syndrome 3 = 00(X)
       LBECR0          00AA2214
                                       Command Address =  = 000AA2214
       LBECR1          00038040
                                       CMD during error = Read ---------------
                                       CNF was asserted for this command
                                       Shared was asserted for this cmd.
                                       Dirty was asserted for this cmd.
                                       CMD/Address Parity = 01(X)
                                       Cmder ID REQ&lt;3:0&gt; = 00(X)
                                       Data Cycle Error = 00(X)
       LMODE           000332A4
                                       4M-Byte
                                       Invalidate B-Cache ------------------
                                       NVAX+ 8k 2 sets I-Cache=2k VIC
                                       Inhibit writes to STx_C
                                       cnt 16 STx_C before LSB LOCKOUT
                                       Pass 3 LEVI-A
       LLOCK           00E2A090
                                       Address Invalid --------------------
       GB HALT             0038
       GB INTR             0000
       GB PMASK            0001
                                       halt enable
                                       Select UART0A local terminal
       GB WHAMI            00E1
                                       1 or more CPUs have GBus$LEDs asserted
                                       LSB Node ID = 01(X)
       ECR             00120002
                                       fbox enable
                                       pmf pmux   = 01
                                       pmf emux   = 02
       VPSR            00000000
       VAER            00000000
                                       Vect Dest Reg Mask = 0000(X)
       VMAC            00000000
       BIU CTL         AFE09FF8
                                       external cache enable
                                       Generate/Expect ECC on check_h pins
                                       output enable of cache rams
                                       2-way associative
                                       2X CPU Cycle
                                       IO Map = 03(X)
                                       4 Mbytes
       BC TAG          1FC13800
                                       tag_match
                                       tag control V
                                       tag control D
                                       tag P
                                       BC TAG = 0FE0(X)
       BIU STAT        F00E0070
                                       Bits 33,32 BIU Addr Reg = 03(X)
                                       Bits 33,32 Fill Addr Reg = 03(X)
       BIU ADDR        00000298
       FILL SYN        00000000
                                       Lo ECC Syn bits Low Longword = 00(X)
                                       Hi ECC Syn bits High Longword = 00(X)
       FILL ADDR       000002A8
       VMAR            000007E0
                                       Sub Block Select = 00(X)
                                       Row Index = 3F(X)
                                       Error Address Field = 00000000(X)
       VTAG            03520586
       VDATA           53D655D6
       ICSR            00000001
                                       enable VIC
       PAMODE          00000001
                                       32 bit physical address mode
       MMEADR          02B23200
       MMEPTE          00000000
       MMESTS          18008000
                                       MMESTS Lock Bits Not Set
       TBADR           00000000
       TBSTS           800001D0
                                       TBSTS.LOCK&lt;0&gt; NOT SET
       PCADR           FFFFFFF8
       PCSTS           FFFFF800
                                       PCSTS.LOCK&lt;0&gt; NOT SET
       PCCTL           FFFFFC13
                                       D-stream enabled
                                       I-stream enabled
                                       parity checking enabled
                                       Performance Monitor Mode = 00(X)
 
 LSB SUBPACKET
       PHYS ADDR       00000000
                       00000000
 
 ******************************* ENTRY       4. *******************************
 ERROR SEQUENCE 38991.                           LOGGED ON:        SID 17000201
 DATE/TIME 30-JUN-2000 07:34:58.23                            SYS_TYPE 01420201
 SYSTEM UPTIME: 4 DAYS 18:21:08
 SCS NODE: TAIT                                                VAX/VMS V6.2
 
 INT60 ERROR KA7AA-AA  CPU FW REV# 1.  CONSOLE FW REV# 4.2
       PACKET REV      00000002
       RESERVED        00000000
 
       SW FLAGS        00008000
                       00000000
                       00100000
                       00000000
       LOGGING OFF     00000000
                       00000000
                       00000000
                       00000000
       ACTIVE CPUS     00000007
       HW REVISION     00000000
       SYS SERIAL NUM  00005651
                       00000000
                           0000
                                       SYS SERIAL NUM = QV........
       SERIAL NUMBER   30365941
                       36303336
                           3330
                                       SERIAL NUMBER = AY60630603
       RESRC DISABLE   00000000
 
       PHYS ADDRESS    F8000000
                       00000000
       LDEV            00028002
                                       Laser NVAX Processor, 4M
                                       Device Revision = 02(X)
       LBER            00000000
       LCNR            00000001
                                       Enable Correctable Err Detection
                                       Self Test Passed
       LMERR           00000000
       LMMR6           00000381
                                       Enable output
                                       interleaved modules = 1, compare bits 0
                                       Interleave Address = 00(X)
                                       Address Width = 0C(X)
                                       banks per mod = 2, bits in bank = 1
                                       Module address = 00000000(X)
       LMMR7           00100381
                                       Enable output
                                       interleaved modules = 1, compare bits 0
                                       Interleave Address = 00(X)
                                       Address Width = 0C(X)
                                       banks per mod = 2, bits in bank = 1
                                       Module address = 00000008(X)
       LBESR0          0000000C
                                       Syndrome 0 = 0C(X)
       LBESR1          0000000C
                                       Syndrome 1 = 0C(X)
       LBESR2          0000000C
                                       Syndrome 2 = 0C(X)
       LBESR3          0000000C
                                       Syndrome 3 = 0C(X)
       LBECR0          00400036
                                       Command Address =  = 000400036
       LBECR1          00008020
                                       CMD during error = Read CSR
                                       CNF was asserted for this command
                                       CMD/Address Parity = 00(X)
                                       Cmder ID REQ&lt;3:0&gt; = 00(X)
                                       Data Cycle Error = 00(X)
       LMODE           000332A4
                                       4M-Byte
                                       Invalidate B-Cache
                                       NVAX+ 8k 2 sets I-Cache=2k VIC
                                       Inhibit writes to STx_C
                                       cnt 16 STx_C before LSB LOCKOUT
                                       Pass 3 LEVI-A
       LLOCK           00F7A134
                                       Address Invalid
       GB HALT             0038
       GB INTR             0000
       GB PMASK            0009
                                       halt enable
                                       Select UART0A local terminal
       GB WHAMI            00E0
                                       1 or more CPUs have GBus$LEDs asserted
                                       LSB Node ID = 00(X)
       ECR             00000002
                                       fbox enable
                                       pmf pmux   = 00
                                       pmf emux   = 00
       VPSR            00000000
       VAER            00000000
                                       Vect Dest Reg Mask = 0000(X)
       VMAC            00000000
       BIU CTL         AFE09FF8
                                       external cache enable
                                       Generate/Expect ECC on check_h pins
                                       output enable of cache rams
                                       2-way associative
                                       2X CPU Cycle
                                       IO Map = 03(X)
                                       4 Mbytes
       BC TAG          1E819000
                                       tag control V
                                       tag control P
                                       tag P
                                       BC TAG = 0F40(X)
       BIU STAT        30080370
                                       ECC ERR. ON EXT. CACHE FILL DATA
                                       FILL ECC ERROR WAS CORRECTABLE
                                       dread
                                       Fill Quadword in Error = 00(X)
                                       Bits 33,32 BIU Addr Reg = 03(X)
                                       Bits 33,32 Fill Addr Reg = 00(X)
       BIU ADDR        00000298
       FILL SYN        00003800
                                       Lo ECC Syn bits Low Longword = 00(X)
                                       Hi ECC Syn bits High Longword = 70(X)
       FILL ADDR       15444298
       VMAR            000007E0
                                       Sub Block Select = 00(X)
                                       Row Index = 3F(X)
                                       Error Address Field = 00000000(X)
       VTAG            03520586
       VDATA           53D655D6
       ICSR            00000001
                                       enable VIC
       PAMODE          00000001
                                       32 bit physical address mode
       MMEADR          02EE08FC
       MMEPTE          00000000
       MMESTS          1C008000
                                       MMESTS Lock Bits Not Set
       TBADR           00000000
       TBSTS           800001D0
                                       TBSTS.LOCK&lt;0&gt; NOT SET
       PCADR           FFFFFFF8
       PCSTS           FFFFF800
                                       PCSTS.LOCK&lt;0&gt; NOT SET
       PCCTL           FFFFFC13
                                       D-stream enabled
                                       I-stream enabled
                                       parity checking enabled
                                       Performance Monitor Mode = 00(X)
 
 
 
 The Answer is:
 
  Please contact your hardware service organization directly.
 
