  problem locking down more than 8 megabytes? 
 The Question is:
 
I've recently migrated four openvms/axp 6.2 device
drivers to OpenVMS 7.1.  I followed Lenny S. example
for calling the exe_std$lock_err_cleanup when a
a buffer can not be locked down.  In fact
everything works just fine unless I try to
lock down greater than 8Mb for the transfer.
 
Question:  Any release notes or bug fixes
for this routine?  The page_lock_failure
routine is called and the irp to irpe to irpe
are correctly threaded.  The all looks good
in the page_lock_failure routine.
 
I understand that you do not intend to debug
drivers or crash dumps, but can someone check to
see if there are any reports from others.  I have
the IRP and IRPEs from the kernel debugger.
 
 
 The Answer is:
 
  Please contact the customer support center for assistance.
 
