  Problems changing nodename and address? (TCP/IP) 
 The Question is:
 
Was recently upgraded from DECnet Phase IV to Phase V.  Every time I change
the DECnet node name and node number on a newly installed machine (image
copy of a currently running MicroVAX, same model as the new one).  I run
NETCONFIG (Phase IV) or NET$CONFI
GURE to change these values, then run MC SYSGEN and change them in scsnode
and scssystemid, then reboot.  After the reboot, all TCP/IP connectivity
disappears (cannot even ping the box).  The host name defined earlier using
UCX$CONFIG is the same as the n
ew node name I am trying to configure.  I read FAQ on how to change the node
name, but see nothing on how to change node number/address.  HELP!!
 
 
 The Answer is:
 
  The OpenVMS Wizard would recommend performing the NETCONFIG or NET$CONFIG
  pass and the UCX$CONFIG or TCPIP$CONFIG pass in the context of the target
  system -- and not on another system.  (This will ensure that the device
  names and other system-specific configuration details are correct for the
  target system.)
 
  Please contact the Compaq Customer Support Center for further assistance.
 
