  Reconfiguring DSSI hardware? 
 The Question is:
 
I have to remove the 2nd alpha 4100 Server and
the Vax4000-300, so it leaves me just 1 Alpha4100 server which i connect (dssi)
 to the
Sw800 first Hscp01 controller.
 
1) Question:
As the Vax is removed from the 2nd controller
do I need to terminate this 2nd controller   port, or can i leave it open and
 still be dual redundant with only one controller connected
with 1 alphaServer 4100.
 
Kind Regards
Ferry Eden Commerzbank (Nederland) N.V. Amsterdam.
 
 The Answer is :
 
  Yes, a DSSI bus does require proper termination.  That said, there are
  a variety of ways that DSSI buses and DSSI controllers can be connected.
  Please contact your hardware support organization for assistance in
  reconfiguring your DSSI bus and your system hardware.
 
 Answer written or last revised on  6-MAY-2002 
