  LAT vs (TCP) IP Programming? 
 The Question is:
 
Differences between Lat sys$qio and TCP/IP
sys$qio?
 
 
 The Answer is :
 
  Yes, there are many differences between the LAT (LTDRIVER) device
  driver interface and the various IP APIs and this includes the API
  for the BGDRIVER interface.  For details on the respective APIs,
  please consider reading the documentation for the respective APIs.
 
  Please also consider reading through at least some of the following
  existing discussions:
 
    (546), (2312), (2407), (2631), (2696), (3202), (3280), (5173),
    (6447), (7504), likely others.
 
  For discussions of LAT and IP (telnet and LPR/LPD printing), please
  see the topics and drivers and print symbiont details discussed in
  topic (8177) and the notes referenced there.  This includes:
 
  See (546), (1020), (1370), (1679), (1938), (2312), (2631), (2696),
  (3041), (3250), (3202), (3280), (4394), (5173), (5737), (5881),
  (6271), (6467), (7143), (7151), (7530), (7959), and other topics.
 
 
 Answer written or last revised on  30-JUN-2003 
