  Hardware Self-Test Errors, Diagnostics? 
 The Question is:
 
Is there a manual that defines the errors at boot for a VAX 3100 model 98. I am
 getting an error and a screen dump of messages at the countdown number 19.
 
KA59-A V2.1, VMB 2.16
Performing normal system tests.
71..70..69..68..67..66..65..64..63..62..61..60..59..58..57..56..
55..54..53..52..51..50..49..48..47..46..45..44..43..42..41..40..
39..38..37..36..35..34..33..32..31..30..29..28..27..26..25..24..
23..22..21..20..19..
 
? Test_Subtest_5F_02  Loop_Subtest=00  Err_Type=FF   DE_SGEC.lis
Vec=0000    Prev_Errs=00   P1=05000001   P2=00000000   P3=00000000  P4=00000000
P5=00000000  P6=00000000   P7=00000000   P8=00000000   P9=00000000 P10=0000009A
Stat=0084  FRU=1  LED=9A  Ext_Stat 00000001 00000000 00000000 00004008 1FF8B7B4
 1FF8C3E8
 dser=0000 cesr=00000000 intmsk=00 icsr=01 pcsts=0000 pcctl=FE13 cctl=00000027
 bcetsts=0000 bcedsts=0000 cefsts=00019200 nests=00 mmcdsr=00000000
 mesr=00000000
 
18..17..16..15..14..13..12..11..10..09..08..07..06..
 
? Test_Subtest_53_09  Loop_Subtest=00  Err_Type=FF   DE_SSC_TOY_Clock.lis
Vec=0000    Prev_Errs=01   P1=00000001   P2=00048600   P3=80048696  P4=00D55570
P5=00000000  P6=00000000   P7=00000000   P8=00000000   P9=00000000 P10=00000000
r0=00000002  r1=20140110   r2=87506E83   r3=0002CAE9   r4=87506E8D  r5=200585C4
r6=000000A0  r7=00090CA0   r8=0000000A   r9=20140758  r10=00000010 r11=1FF1EC00
 dser=0000 cesr=00000000 intmsk=00 icsr=01 pcsts=0000 pcctl=FE13 cctl=00000027
 bcetsts=0000 bcedsts=0000 cefsts=00019200 nests=00 mmcdsr=00000000
 mesr=00000000
 
05..04..03..
Normal operation not possible.
 
 
 The Answer is :
 
  Please contact your hardware support organization for assistance with
  hardware-level errors, such as the motherboard-level network hardware
  failure reported by test 5F (Test_Subtest_5F_02) and the time of year
  clock failure reported by test 53 (Test_Subtest_53_09).  The typical
  FRU for both 5F and for 53 failures is the system motherboard.
 
  For pointers to the available hardware documentation, please see the
  OpenVMS FAQ, and particularly the hardware documentation pointers and
  (if you wish to perform self-maintenance of your systems) the Assisted
  Services program for access to diagnostics and service manuals.
 
  Again, please contact your hardware service organization for console
  errors and hardware-level errors.
 
 Answer written or last revised on  24-NOV-2003 
