  no baud puns here 
 The Question is:
 
How do I set the baud rate on the DSW42.
It seams to be defaulting to 19.2.  I need
it to be 9600.
thanks
 
 The Answer is:
 
  For asynchronous serial line devices, please see HELP SET TERMINAL,
  particularly looking at the /PERMANENT and /SPEED qualifiers.
 
  One often finds SET TERMINAL commands included in SYSTARTUP_VMS.COM
  or another component procedure of the local system startup.
 
  For information on resetting the speed on a synchronous communications
  card, please see the documentation for the specific module in question,
  and for the software package and/or device driver(s) that support it.
 
  For assistance with the module and the module settings, please contact
  your hardware support organization.
 
