  SET HOST to HSJ controller? 
 The Question is:
 
what is the vms command to connect to hsj013 or other devices as far as RAID is
 concerned?
 
 The Answer is:
 
  Usually some variant of SET HOST/DUP, depending on the particular
  widget involved.
 
  Please see the OpenVMS FAQ for information on SET HOST/DUP and
  related commands.
 
