  TCP/IP (UCX) UCX$LPD_VMS_FLAGPAGES? 
 The Question is:
 
How to reproduce OpenVMS print seperater
under UCX LPR print queues?
According to the manual, System Logical
UCX$LPD_VMS_FLAGPAGES can be defined to
request the UCX_SMB to generate the OpenVMS
flags.  However, it does not work.
Please provide detail steps.
 
 
 The Answer is:
 
  Please upgrade to the appropriate TCP/IP Services for OpenVMS, and
  apply the associated ECO kit.  Release notes circa V3.3 included a
  write-up on the use of UCX$LPD_VMS_FLAGPAGES, including interactions
  with inbound and outbound jobs, as well as with UCX$LPRSETUP and the
  steps necessary in UCX$LPD_STARTUP.COM.
 
  Realize that UCX$LPD_VMS_FLAGPAGES is translated only at symbiont
  startup.
 
  If these steps fail to resolve the reported difficulty, please contact
  the customer support center directly.
